[Back to NUMBERS SWAG index] [Back to Main SWAG index] [Original]

    The commands you need to rotate a Byte/Word are:

    ROR, ROL, RCR, RCL.
    ROR ==> Rotates the bits the number of times specified, so that the
            rightmost bits are rotated into the leftmost bits.  NO BITS
            ARE LOST.  ROL is the same thing in the opposite direction.

    RCR ==> Practically the same as the ROR/ROL instruction, but it rotates
            the bit into the carry, and the carry bit is rotated into the
            leftmost bit of the Byte/Word.  {Rotate right through carry}
            RCL is the same in the other direction.

    The format For each of ROR,ROL,RCR,RCL,SHR,SHL is

      [Instruction]  <Destination>  <Shift Count>

    To reWrite your original code:

    Asm
      Mov  AL, ByteVar
      Ror  AL, 1
      Mov  ByteVar, AL
    end

    The above would rotate the bits in the Variable ByteVar by one to the right.

[Back to NUMBERS SWAG index] [Back to Main SWAG index] [Original]