[Back to CRT SWAG index] [Back to Main SWAG index] [Original]

    {****************************************************************************
     * Procedure ..... SetBright;
     * Purpose ....... To enable intensity vice blinking
     * Parameters .... None
     * Returns ....... Nothing
     * Notes ......... Colors with the background attribute high-bit set will
     *                 show the background in bright colors.
     * Author ........ Martin Richardson
     * Date .......... October 28, 1992
     ****************************************************************************}
    PROCEDURE SetBright; ASSEMBLER;
    ASM
       MOV  AX, 1003h
       XOR  BL, BL
       INT  10h
    END;

[Back to CRT SWAG index] [Back to Main SWAG index] [Original]