[Back to EGAVGA SWAG index] [Back to Main SWAG index] [Original]

    {
    AG> Does anyone out there know how to set the screen display for 28 rows, in
    AG> VGA mode?  I've seen this in a couple of programs, and really like it.

    Here goes a small assembly routine to switch the screen to 28-line mode. }

           MOV   AX,1202          ;set up 400 scan lines
           MOV   BL,30
           INT   10
           MOV   AX,0003          ;set up normal text mode
           INT   10
           MOV   AX,1111          ;load ega character set
           MOV   BL,00
           INT   10

[Back to EGAVGA SWAG index] [Back to Main SWAG index] [Original]