[Back to ANSI SWAG index] [Back to Main SWAG index] [Original]

    {
    You can use this routine with or without the CRT unit. All output will
    be routed through the BIOS. You must have the ANSI.SYS driver loaded in
    your config.sys file.

    }
    procedure awrite(c : byte);

    begin
     asm
    mov ah,2;
    mov dl,c;
    int $21;
     end;
    end;

[Back to ANSI SWAG index] [Back to Main SWAG index] [Original]