[Back to CRT SWAG index] [Back to Main SWAG index] [Original]

    {
    >Does anyone know how to clear the screen Really fast ?
    Well, here is some Asm code but I haven't tested it. It should work:
    }

    Procedure FastClrScr; Assembler;
    Asm
      MOV AH,0Fh
      INT 10h
      MOV AH,0
      INT 10h
    end;

    begin
      FastClrScr;
    end.

[Back to CRT SWAG index] [Back to Main SWAG index] [Original]