[Back to CURSOR SWAG index] [Back to Main SWAG index] [Original]

      Procedure HideCursor;  assembler;
      asm
        mov      ah,$01  { Function number }
        mov      ch,$20
        mov      cl,$00
        Int      $10     { Call BIOS }
      end;  { HideCursor }

      Procedure RestoreCursor;  assembler;
      asm
        mov      ah,$01  { Function number }
        mov      ch,$06  { Starting scan line }
        mov      cl,$07  { Ending scan line }
        int      $10     { Call BIOS }
      end; { RestoreCursor }

[Back to CURSOR SWAG index] [Back to Main SWAG index] [Original]