[Back to JOYSTICK SWAG index] [Back to Main SWAG index] [Original]

    Anyone know how to read the Joystick....

    if you are using an AT (286 or later), here's the easy way.
    Use Intr ($15, Regs), and load AH With the $84, then load
    DX With 1 to get the joystick status' and 0 to get the
    button status.  if you use DX=1, it returns:

    AX x of joystick A
    BX y of joystick A
    CX x of joystick B
    DX y of joystick B

    if you use DX=0:

    AL button status, bit #
       4 joystick A,button 1
       5 joystick A,button 2
       6 joystick B,button 1
       7 joystick B,button 2

[Back to JOYSTICK SWAG index] [Back to Main SWAG index] [Original]