[Back to UNITINFO SWAG index] [Back to Main SWAG index] [Original]

    Provided you have a copy of Borland Pascal 7.0, you can Single-step, trace
    into, put breakpoints etc. in routines contained in SYSTEM.TPU.

    to do so, you must take the following steps:
    -  Extract all Files from RTLSYS.ZIP
    -  Assemble all .Asm Files With the following switches:

       TAsm *.Asm /mx /zi

    (Ignore the Single error, as well as all warnings)

    -  Compile SYSTEM:

       BPC SYSTEM /$D+ /$L+

    -  Add the directory wherein you keep the .Asm Files to the inCLUDE directories
    list of BPC.CFG and/or the "Options/Directories" of the IDE.
    That's it.  The benefits are enormous, especially it you do a lot of debugging
    with a stand-alone debugger (TD, TD286 or TD386).  Like I used to do -- Until I
    discovered the joy of using the new IDE of BP 7.  Well, too late the hero, I
    guess...

[Back to UNITINFO SWAG index] [Back to Main SWAG index] [Original]