[Back to SOUND SWAG index] [Back to Main SWAG index] [Original]

    {
    => A few days ago you posted a VOC file player that doesn't use CT-VOICE.DRV.
    => I would like to know how to use it.  So far I have tried this.
    => Uses PLAY;
    =>
    => Var A : Pointer;
    =>
    => Begin
    =>  PLAY_VOC('HI.VOC',A); End.
    => End.
    =>
    => Could you explain why this doesn't work and or give me a working demo!

    You have to use "getmem" to reserve some memory before calling "play_voc".
    Here follows a slightly modified unit + demo...

    Alwin Loeckx - fido (2:291/754.6)
    }

    unit play;

    interface

    { resetdsp returns true if reset was successful }
    { base should be 1 for base address 210h, 2 for 220h etc... }
    function reset_dsp(base : word) : boolean;

    { write dac sets the speaker output level }
    procedure write_dac(level : byte);

    { readdac reads the microphone input level }
    function read_dac : byte;

    { speakeron connects the dac to the speaker }
    function speaker_on: byte;

    { speakeroff disconnects the dac from the speaker, }
    { but does not affect the dac operation }
    function speaker_off: byte;

    { functions to pause dma playback }
    procedure dma_pause;
    procedure dma_continue;

    { playback plays a sample of a given size back at a given frequency using }
    { dma channel 1. the sample must not cross a page boundry }
    procedure play_back(sound : pointer; size : word; frequency : word);

    { plays voc-file }
    procedure play_voc(filename : string; buf : pointer);

    { true if playing voc }
    function playing_voc : boolean;

    implementation

    uses crt;

    var dsp_reset        : word;
        dsp_read_data    : word;
        dsp_write_data   : word;
        dsp_write_status : word;
        dsp_data_avail   : word;

        since_midnight   : longint absolute $40:$6C;
        playing_till     : longint;

    function reset_dsp(base : word) : boolean;

    begin
     base := base * $10;

     { calculate the port addresses }
     dsp_reset        := base + $206;
     dsp_read_data    := base + $20a;
     dsp_write_data   := base + $20c;
     dsp_write_status := base + $20c;
     dsp_data_avail   := base + $20e;

     { reset the dsp, and give some nice long delays just to be safe }
     port[dsp_reset] := 1;
     delay(10);

     port[dsp_reset] := 0;
     delay(10);

     reset_dsp := (port[dsp_data_avail] and $80 = $80) and
                  (port[dsp_read_data] = $aa);
    end;

    procedure write_dsp(value : byte);

    begin
     while port[dsp_write_status] and $80 <> 0 do;
     port[dsp_write_data] := value;
    end;

    function read_dsp : byte;

    begin
     while port[dsp_data_avail] and $80 = 0 do;
     read_dsp := port[dsp_read_data];
    end;

    procedure write_dac(level : byte);

    begin
     write_dsp($10);
     write_dsp(level);
    end;

    function read_dac : byte;

    begin
     write_dsp($20);
     read_dac := read_dsp;
    end;

    function speaker_on: byte;

    begin
     write_dsp($d1);
    end;

    function speaker_off: byte;

    begin
     write_dsp($d3);
    end;

    procedure dma_continue;

    begin
     playing_till := since_midnight + playing_till;
     write_dsp($d4);
    end;

    procedure dma_pause;

    begin
     playing_till := playing_till - since_midnight;
     write_dsp($d0);
    end;

    procedure play_back(sound : pointer; size : word; frequency : word);

    var time_constant : word;
        page          : word;
        offset        : word;

    begin
     speaker_on;

     size := size - 1;

     { set up the dma chip }
     offset := seg(sound^) shl 4 + ofs(sound^);
     page := (seg(sound^) + ofs(sound^) shr 4) shr 12;
     port[$0a] := 5;
     port[$0c] := 0;
     port[$0b] := $49;
     port[$02] := lo(offset);
     port[$02] := hi(offset);
     port[$83] := page;
     port[$03] := lo(size);
     port[$03] := hi(size);
     port[$0a] := 1;

     { set the playback frequency }
     time_constant := 256 - 1000000 div frequency;
     write_dsp($40);
     write_dsp(time_constant);

     { set the playback type (8-bit) }
     write_dsp($14);
     write_dsp(lo(size));
     write_dsp(hi(size));
    end;

    procedure play_voc(filename : string; buf : pointer);

    var f : file;
        s : word;

        freq : word;

        h : record
             signature  : array[1..20] of char; { vendor's name }
             data_start : word;                 { start of data in file }
             version    : integer;              { min. driver version required }
             id         : integer;              { 1 - complement of version field
    +$1234 }        end;                                { used to indentify a .voc
    file }
        d : record
             id   : byte;                { = 1 }
             len  : array[1..3] of byte; { length of voice data (len data + 2) }
             sr   : byte;                { sr = 256 - (1,000,000 / sampling rate) }
             pack : byte;                { 0 : unpacked, 1 : 4-bit, 2 : 2.6 bit, 3:
    2 bit packed }        end;

    begin
     {$i-}
     if pos('.', filename) = 0 then filename := filename + '.voc';

     assign(f, filename);
     reset(f, 1);

     blockread(f, h, 26);

     blockread(f, d, 6);

     freq := round(1000000 / (256 - d.sr));
     s    := ord(d.len[3]) + ord(d.len[2]) * 256 + ord(d.len[1]) * 256 * 256;

     (*
     writeln('-----------header----------');
     writeln('signature: ', h.signature);
     writeln('data_start: ', h.data_start);
     writeln('version: ', hi(h.version), '.', lo(h.version));
     writeln('id: ', h.id);
     writeln;
     writeln('------------data-----------');
     writeln('id: ', d.id);
     writeln('len: ', s);
     writeln('sr: ', d.sr);
     writeln('freq: ', freq);
     writeln('pack: ', d.pack);
     *)

     blockread(f, buf^, s);

     close(f);
     {$i-}

     if ioresult <> 0 then
      begin
       writeln('Can''t find voc file "' + filename + '"');
       halt(1);
      end;

     playing_till := since_midnight + round(s / freq * 18.20648193);
     play_back(buf, s, freq);
    end;

    function playing_voc : boolean;

    begin
     playing_voc := since_midnight > playing_till;
    end;

    begin
     if not reset_dsp(2) then
      begin
       writeln('SoundBlaster not found at 220h');
       halt(1);
      end
     else
      writeln('SoundBlaster found at 220h');
    end.

    { -----------------"demo.pas"------------------------------------------ }

    uses crt, play;

    var voc  : pointer;
        name : string;

    begin
     getmem(voc, 65535);

     if paramcount = 1 then
      name := paramstr(1)
     else
      begin
       write('Play voc file (size < 65535!): ');
       readln(name);
      end;

     play_voc(name, voc);
     writeln;

     writeln('Playing, press "P" to pause...');

     repeat
      if keypressed then if (upcase(readkey) = 'P') then
       begin
        dma_pause;

        writeln('Press "C" to continue...');

        repeat
        until upcase(readkey) = 'C';

        writeln('Continuing...');
        dma_continue;
       end;
     until playing_voc;

     writeln('Done...');

     freemem(voc, 65535);
    end.

[Back to SOUND SWAG index] [Back to Main SWAG index] [Original]