[Back to CRT SWAG index] [Back to Main SWAG index] [Original]

     KF> Is there a way that I can display Char #7 on the screen without the
     KF> beep? I'm trying to create an ASCII chart to go with a text font editor
     KF> I've written, but this character (and one or two others) keep me from
     KF> being able to display all 256 ASCII symbols. Please help...

     simple!

      mem[$b800:X*2+Y*160]:=7;
      mem[$b800:x*2+Y*160+1]:=attribute;

[Back to CRT SWAG index] [Back to Main SWAG index] [Original]