[Back to FAQ SWAG index] [Back to Main SWAG index] [Original]

    SECTION 6 - Protected Mode Programming

    This document contains information that is most often provided
    to users of this section.  There is a listing of common
    Technical Information Documents that can be downloaded from the
    libraries, and a listing of the five most frequently asked
    questions and their answers.

    TI1184   Overview of Borland Pascal 7.0 and Turbo Pascal 7.0
    TI1722   Declaring an array on the heap
    TI1760   Creating a  temporary stack in real or protected mode
    TI1188   Creating protected mode apps with Borland Pascal
    TI1171   Problem Report Form
    TI1719   Booting Clean

    NEWRTM.ZIP   Latest RTM.EXE and DPMI16BI.OVL
    PASALL.ZIP   Collection of Technical Information sheets from
                 1986 on
    EZDPMI.ZIP   Unit encapsulating all common DPMI requirements for
                 protected mode programming
    BIGSTU.PAS   How to cope with memory allocations > 64K
    MOUSE.ZIP    General Purpose mouse unit for text/graphics mode

    Q.   "When using the BP7 IDE to compile a protected mode
         application, how do I step through the code like I do with
         real mode applications?"

    A.   To debug protected mode programs, you must use the external
         debugger (TDX).  You can put it on the TOOLS menu to make
         it just a keystroke away.

    Q.   "When I convert a program from Real Mode to Protected Mode,
         do I have to change the GetMem calls to GlobalAlloc and
         GlobalDiscard?"

    A.   No, you don't have to change the GetMem calls.  GetMem is a
         better allocation method.  Getmem will do a better job of
         allocating memory. It allocates the memory in 8K chunks,
         then suballocates from that. The reason for this is that
         there are a maximum of 2000 selectors availble in BP7, so
         you don't want to waste them. GlobalAlloc calls the DPMI
         directly to allocate the memory, bypassing the heap manager.
         GlobalAlloc is there for when you need to bypass the heap
         manager for some reason, but you normally don't want to do
         that.

    Q.   "How do I profile a protected mode application using BP7?"

    A.   You can only profile real mode applications, Borland does
         not supply a protected mode profiler.

    Q.   "I have ported a large program to protected mode and am
         getting a General Protection Fault on calls to GetMem.  What
         could be causing this?"

    A.   In DPMI, a Local Descriptor Table (LDT) can contain 8192
         selectors.  The Run Time Manager (RTM) maintains an
         internal table to track allocated selectors.  The RTM table
         has a capacity of approximately 2K selectors.  GlobalAlloc
         and GetMem calls that need to allocate a new block will fail
         when that 2K table is full.

    Q.   "I have a protected mode application that was created with
         BP7. When running the program in a DOS box under Windows,
         the computer locks up.  What could be causing this?"

    A.   Check the "XMS KB Required" and "XMS KB Limit" settings in
         the .PIF file used for the DOS box.  The "Required" setting
         should be 0 and the "Limit" should be at least 2048K.

[Back to FAQ SWAG index] [Back to Main SWAG index] [Original]